The file format between the UE and Server is following

START\_MSG

TIME=77 1f 2b 51 87 c6 c2 00

MSGID=1007

GUIDINFO=ABCDEFGHIJK

LAT=1234567.123450

LONG=1234567.123400

ALT=1234567.123400

SPEED=100

DIR=1231

LOCACY=89

MSGBUFF=00 00 05 00 00 00 00 02 41 00 01 01 07 06 00 00 00 01 06 00 00

END\_MSG

START\_MSG represent the start of log message

TIME represent the time at that time device has capture this log

MSGID represent the message Identifier. The detail of message identifier is define in interface document

GUIDINFO is provided by application

LAT is latitude of the UE

LONG is longitude of the UE

ALT represent the altitude of the UE

SPEED provide the speed of the UE

DIR represent the direction on which UE is moving

LOCACY represent the location accuracy

MSGBUFF represent the message buffer that was captured by DM library

END\_MSG represent the end of message